2. Specification of Bulbs 
	Type


	Specification


	Headlamp


	12V 55W



	Turning lamp, rear foglamp, reverse lamp


	12V 21W



	License plate, side turning and high-mounted stop lamp


	12V 5W



	Stop lamp


	12V 21W



	Position lamp


	12V 5W



	Front foglamp


	12V 55W



	Front/rear ceiling lamp


	12V 8W




6. Removal and Installation of Front Foglamp

	1) Dismantle the front bumper.

a. Dismantle the fixing bolts under front bumper. 
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	b. Dismantle the side fixing bolts of front bumper. 
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	c. Dismantle the connecting bolts of front wheel house at both sides. 
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	d. Dismantle the three fixing bolts at the top of front bumper. 

e. Remove the bumper with attention to the top clips at both sides. Unplug the wiring harness for the two foglamps in front. 

Note: Please don’t overexert while taking out the wiring harness as well as plug for the foglamp. 
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	2) Dismantle front foglamp from the bumper.
  Dismantle the three nuts as shown by the arrow by open wrench, and remove the foglamp assembly from the front of the bumper. 
3) Install in the reversed sequence.
Torque: 
Fixing of front foglamp 2.0±0.2 Nm  

Q32006 (3 pcs)
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Fixing bolt








Fixing Nut








